These '.bin' are either 3D LUTs or Heat Tables for various HiTi
printers.  All files were extracted from public HiTi source code or
binary driver releases.

LUT filename Codes:

 C M Q P ? ra [ .bin ]
           --  model code, see below
         -     media version, 0..n (if not present, interpret as 0)
       -       always P (or 'CL', or 'B')
     -         print quality, Q == fine, P == normal
   -           media type, M == DNP, C == CHC         (?)
 -             Always C

  model codes:

    cb = CS2xx
    ra = P51x
    rd = P72x
    rh = P75x
    ri = P52x (or 'ri1')
    rk = P530
    si = P11x

Heat table codes:

 hea 0 q c ra [.bin]
           -- model code, see above
         -    media type, h == DNP, c == CHC      (?)
       -      print quality, q == fine, t == normal, (or p == ?)
     -        media version, 0..n (or 't')
  ---         always 'hea'

Heat table types:

  size

  11108    (SEHT2 * 5 + CVD (Y + M + C + Gloss + Matte + CVD)
  12568    ??
  12603    ??
  15732    ??
